How to flash EC firmware:

1. Plug in AC adaptor.
2. Run ECFlash2.bat under pure DOS to start EC flash procedure, the system will shut down automatically when the procedure is finished.
3. Plug off AC adapter for 5 seconds then plug in AC adapter.
4. Power on system and enter CMOS setup to check EC firmware version.


